There are 2 files in this directory, External.bin and Internal.bin

These are encrypted binary files that can be used by the bootloader to program a new application.

To utilize these files (Internal/External.bin), copy them into the home directory of the SD card and insert back into the SuRG unit.

* Turn off power to the SuRG unit
* wait 10+ seconds
* Turn on power to the SuRG unit

The boot loading process will begin.

This will program the application in internal.bin and external.bin into the SuRG unit.
